**B11**--Reference OCXO, aging 2 × 10–7/year

**B21**--Universal signaling unit; includes signaling module for AMPS, TDMA, GSM/GPRS/EGPRS

**B41**--Audio generator and analyzer; includes audio frequency (AF) generator, voltmeter, distortion meter

**B52**--Internal versatile multimode speech coder/decoder; R&S CMU-B21 necessary

**B54**--Signalling module for AMPS, TDMA, GSM/GPRS/EGPRS; R&S CMU-B21 necessary

**B55-**-HD option for (E)GPRS application testing with more than 2 UL slots

**B56-**-WCDMA (3GPP FDD) signaling module for R&S CMU-B21 model 14

**B66**--Versatile baseband board for WCDMA (3GPP FDD) Layer 1, DL, non-signalling

**B68**--Versatile baseband board for WCDMA (3GPP FDD) layer 1, DL and UL, non-signaling

**B95**--Auxiliary generator that covers the requirements of present BCCH by GSM/GPRS/EGPRS and application testing for (E)GPRS

**K47**--R&S Smart Alignment for all GSM and CDMA2000 packages

**K53**--Bluetooth test software

**PK100**--Software package for R&S CMU200 including GSM/GPRS/EGPRS + WCDMA+ CDMA2000 1xRTT + 1xEV-DO + AMPS + IS-136(R&S CMU-PK20, -PK60, -PK80, -PK800, -K27, -K28, -K43, -K88)